Pos. 0 Acoustic wall and ceiling panels

Richter Acoustic-Lightboard® with MR 050 250 V micro-perforations.

Specifications:

front: Micro-perforations at 0.5mm in diameter spaced at 2.5mm on center. Second

series of Micro Perforations set in between the first micro-perforations and offset 45 degrees resulting in the rows spaced at 1.25mm on center. The micro perforations are from edge to edge of the acoustic panel.

core: Acoustically tuned honeycomb core with a rigid perimeter frame at 25mm or 50mm in width.

back: RU 0510 perforations. 5mm diameter at 10mm center to center. 50mm un-perforated border at all four edges.

*Finish option 1. Specifier to select preference.*

finish: front: 0.5mm HPL surface. Manufacturer: xxxxxxxxxxxxxxx

Color/pattern: xxxxxxxxxxxxxxxx

edges: ABS edgebanding to match HPL selection at 0.4mm to 2mm in thickness.

back: HPL balancing sheet for panel stability.

*Finish option 2. Specifier to select preference.*

finish: front: Grade A 0.5mm thick wood veneer laminated to 0.4mm thick CPL

carrier.

Veneer: xxxxxxxxxxxxxxxxxxxx

Veneer cut: xxxxxxxxxxxxxxxxxxxx

Veneer match: xxxxxxxxxxxxxxxxxxxxx

Clear finished.

edges: Wood veneer to match selected species of face veneer. 0.6mm to 2mm in thickness. Clear finished.

back: Grade C balancing veneer for panel stability.

Primed only.

Formats:

Width: 25mm up to 1550mm. Additional widths on request.

Length: 304mm up to 4000. Additional lengths on request.

Thickness: 16mm, 19mm. Optional thicknesses on request.