**Pos. 000** **Richter akustik & design GmbH & Co. KG**

**LightBeton Retro**

Standard Dimensions: 2650 x 1020 mm (104.33” x 40.16”)

2050 x 1250 mm (80.7” x 49.21”) (Standard: without edgebanding)

Standard thickness: 4 mm (0.158“)

Lot size: order related, starting at lot 1

Dimensions:

Product construction: - 1.5 mm (0.059”) LightBeton-Layer

- 2.5 mm (0.098”) Flex-Mineral sheet

Quantity: \_\_\_\_\_\_\_\_\_m² UP: \_\_\_\_\_\_\_\_\_ AP: \_\_\_\_\_\_\_\_\_