**Pos. 000** **Richter akustik & design GmbH & Co. KG**

**LightBeton Formwork**

Standard Dimensions: 2.000 x 1.200 mm (78.74“ x 47.24“)  
1.000 x 1.200 mm (39.37“ x 47.24“)  
600 x 1.200 mm (23.62“ x 47.24“)  
500 x 1.200 mm (19.68“ x 47.24“)

(Standard: without edgebanding)

Standard thickness: 19 mm (0.748“) (other thicknesses on request)

Lot size: order related, starting at lot 1

Color type:

System type:

Dimensions:

Product construction: - 1.5 mm (0.059”) LightBeton-Layer with Formwork system milling

- 16 mm (0.629”) fire retardant MDF

- 1.5 mm (0.059”) LightBeton balancing quality

Edge banding: custom made (LightBeton, ABS, Melamine and PP possible)

Edge types: custom made (groove and rabbet millings on request)

Quantity: \_\_\_\_\_\_\_\_\_m² UP: \_\_\_\_\_\_\_\_\_ AP: \_\_\_\_\_\_\_\_\_